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CENTRE FOR DEVELOPMENT OF ADVANCED COMPUTING

A Scientific Society of Ministry of Electronics & IT, Government of India
Vellayambalam, Thiruvananthapuram- 695 033, INDIA

Tel: 0471-2311704,Fax 0471-2311703

 purchase-cpp@cdac.in, www.cdac.in E-Tender Notice

Limited E-Tender Notice

 Centre for Development of Advanced Computing (C-DAC), Thiruvananthapuram invites online bids through e-procurement (http://eprocure.gov.in/eprocure/app) fromeligible bidders for the supply of items as detailed below with the Terms & Conditions in Section 1.

Tender No. :


  CDAC.PHS.HTG055B.131.22-23

Type of Tender:                               Limited Tender - Supply of Goods and Service
Issue of Tender Document :         
Last Date for Receipt of Bids :      
Technical Bid Opening :                 
Commercial Bid Opening :             Will be informed later

Item Details: Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
 C-DAC Thiruvananthapuram, a Scientific Society under the Ministry of Electronics and Information Technology, Govt. of India, invites electronic tender in Two-Bid form towards Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
The successful bidder selected through this tender has to supply 2Nos. of Mobile Cancer Detection Units mentioned in this document. The bidder has to provide 3 year onsite warranty at Goa and Lucknow.

Scope of work

The scope of the work includes the procurement of necessary equipments and fabrication of Mobile Cancer Detection Units on a chassis with length not less than 11M. The specially designed bus will be used as Mobile Cancer Detection unit. The bus will be air conditioned with roof air conditioner and will be comfortable for people travelling in the bus. While the bus is stationary and is being used for disease diagnosis and treatment, the split air conditioners will be operational for the comfort of patients and medical personnel in the bus.  The bus will be equipped with necessary medical and networking equipments for tele consultation. Medical equipments will be powered by a 6KVA UPS which will be charged from local power sources or the built in petrol generator in the vehicle. A 100 liter fresh water tank, a wash basin and a waste water tank for collection of waste water will be built into the bus. The medical equipments and vehicle chassis will be provided by C-DAC Thiruvananthapuram. Refer Annexure-H for the detailed list of equipments to be supplied by C-DAC Thiruvananthapuram. 
The detailed requirement specifications are included in Annexure D of this document. Bidder has to provide technical compliance for these items. The Bidder shall provide 3 year onsite Warranty for the Mobile Unit during the entire contract period. 
The scope of the bidder also includes:

i. Delivery of fabrication material and equipments at site and its installation and fabrication, including loading and unloading shall be the responsibility of the bidder.

ii. The equipment should be installed, tested and commissioned as recommended by the OEM.

iii. All necessary accessories (including supporting base stand, supporting structures, compatible cables, accessories & any additional fixation etc.) which are required for successful installation and commissioning should be supplied by the bidder. Working drawings and mounting/installation procedure for the works should be approved by C-DAC representative.

iv. Provision of all the necessary cables, accessories/equipment’s & its installation/mounting which are required for the commissioning of the supplied items shall be the scope of the bidder.

v. The bidder should list out and quote for any items that have been missed out by the purchaser but essential for installing and commissioning the supplied items. In case, the bidder fails to list out and quote for such items, the responsibility to successfully install and commission the supplied items shall be the scope of the bidder.
Instructions to bidders 
1. The two-bid system will be followed for this tender. In this system, bidder must submit their offer - online in separate covers as explained below: 

a. Cover-1: Technical Bid 
The technical bid documents shall be submitted in pdf format (tech.pdf) 

b. Cover-2: Commercial bid cover should contain the price information in BOQ.xls (BOQ in excel) 

c. Signed & Scanned copy of Commercial Price Declaration (As per Annexure - C) 

Bidder should ensure that all the documents in Cover-1 are duly filled and signed. 
2. Bid should accompany complete and signed copies of Annexures A, B, C, D, E, F& G. 
3. The bidders are required to submit soft copies of their bids electronically on the CPP Portal, using valid Digital Signature Certificates. Bidder should take into account any corrigendum published on the tender document before submitting their bids. 

4. Bidder shall quote in Indian Currency only. 

5. Bids should accompany the filled and signed Tender Document. 

6. The validity of the quotation should be minimum 90 days from the date of opening of technical bid. 

7. Bidder should mention GST total in the GST column of BOQ 

8. The tender document may be downloaded from the website www.eprocure.gov.in 

9. Any queries relating to the tender document and the terms and conditions contained therein should be send to (email id): purchase-cpp@cdac.in
Section 1: General Terms & Conditions 

1. A prospective bidder requiring any clarification on the tender document may submit his queries, in writing, at the mailing address and as per schedule. Prospective bidders are free to raise their queries and responses / corrigendum will be conveyed to all the prospective Bidders (by way of hosting amendments/ clarifications on the website i.e. at (http://eprocure.gov.in/eprocure/app) and no participant would be informed individually about the response of C-DAC. The decision of the C-DAC regarding acceptability of any suggestion shall be final and shall not be called upon to question under any circumstances. The Bidders are advised to visit the aforementioned website on regular basis for checking necessary updates. 

2. The bids prepared by the bidder and all correspondence and documents relating to the Bids exchanged by the Bidder and C-DAC shall be written in English language. Any printed literature furnished by the Bidder may be written in another language so long the same is accompanied by a duly attested English translation in which case, for purposes of interpretation of the Bid, the English translation shall govern. 

3. The bidder/OEM shall provide the layout, manufacturer, model, material specifications, dimensions, brochures, photo catalogues of items quoted along with the bid, if available. Bidder shall contact C-DAC for any clarification regarding the tender requirement. 

4. Bids without documents in support of the pre-qualification criteria given in this tender shall be summarily rejected. 

5. During Technical evaluation, C-DAC may request the shortlisted bidders to make a presentation on their proposal to an Evaluation Committee to be constituted for the purpose at C-DAC Thiruvananthapuram. It is, however, clarified that, subject to other provisions of this document, every bidder will have to comply the minimum technical specifications laid down in the tender document for being qualified technically. To assist in the examination, evaluation and comparison of Bids, C-DAC may at its discretion ask the bidder for a clarification regarding its bid. The clarification shall be given in writing immediately, but no change in the price shall be sought, offered, or permitted. 

6. During Commercial evaluation, the commercial Bids of the technically qualified bidders will only be opened for further processing. The successful bidder is selected based on the total lowest price including taxes and freight charges and any other expenses. 

7. Bidder shall quote in Indian Rupees only. The rates quoted by the bidder shall be firm throughout the contract period and there shall be no upward revision of the rates quoted by the bidder for any reason whatsoever. 

8. GST payable should be shown separately. Total GST Amount shall be shown in GST amount column of BOQ. Otherwise,quoted price will be treated as all inclusive. Input GST invoice shall be submitted at the time of delivery. 

9. The validity of the quotation should be minimum 90 days from the date of opening of technical bid. 

10. In the commercial bid, the bidders should quote the total price for supply and delivery of all items having three-year OEM on-site warranty as per technical specifications. 

11. The quoted price in the BOQ shall be inclusive of all charges. 

12. The bidder is required to submit Agreement certificate with CDAC for Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty. (Tender Ref No.xxx.xxx.000)
13. The bidder should provide one onsite training at Goa and Lucknow without any extra cost. The date of the training program should be finalized with the approval of C-DAC Thiruvananthapuram.
14. Prior approval of CDAC must be obtained before purchase the equipments (Refer Annexure D for equipment list ) for the fabrication of mobile units. 
14. Locations for the Supply: 
The Items covered by this document are required to be Supply, the completed Mobile Unit at Govt. Medical College Goa and KGMU Lucknow at no extra cost
16. Warranty& Maintenance Support: Bidder/OEM should provide comprehensive onsite Warranty for all the items supplied under the BOQ for a period of 3(Three) years, at Goa and Lucknow at no extra cost. 

Bidder/OEM should provide Next Business Day Support for all the sites. Bidder/OEM should submit a separate undertaking on warranty and Next Business Day Support for a period of three years. 

17. Delivery: Delivery should be completed within 150 days from the date of purchase order. The bidder needs to take care of the documentary formalities and permissions required, if any, from any of the Government agencies/ departments. Delivery of material at site including unloading shall be responsibility of the supplier. 

18. Performance Security: 
Within 15 days of the receipt of notification of award of contract, the successful Bidder shall furnish interest free performance security in the form of bank guarantee/DD/FDR for satisfactory execution of the contract. Performance security shall be equal to 3% of the contract in the form of bank guarantee from a nationalized /scheduled bank valid for 60 days beyond the date of delivery. 
19. Payment Terms: 
	Sl. No
	Milestone
	Payment Value
	Supporting Document

	1
	Completion of structure of 2 Mobile Cancer Detection Units
	30%
	Report attested by CDAC Team 

	2
	Procurement of equipments and the fixing of medical equipments
	30%
	Report attested by CDAC Team

	3
	Completion of interior work, exterior painting and sticker work
	20%
	Report attested by CDAC Team

	4
	Handing over of completely built 2 Mobile Cancer Detection Units
	10%
	Report attested by CDAC Team

	3
	End of contract end. ie, on completion of warranty period of 3 year
	10%
	Report attested by CDAC Team


20. Liquidated Damages shall be levied @0.5% of the total order value, per week per part of the week for the delayed period subject to a maximum of 10% of the order value. 

21. Force Majeure: C-DAC may consider relaxing the penalty and delivery requirements, as specified in this document, if and to the extent that, the delay in performance or other failure to perform its obligations under the contract is the result of an Force Majeure. Force Majeure is defined as an event of effect that cannot reasonably be anticipated such as acts of God (like earthquakes, floods, storms etc.), acts of states / state agencies, the direct and indirect consequences of wars (declared or undeclared), hostilities, national emergencies, civil commotion and strikes at successful Bidder’s premises or any other act beyond control of the bidder. 

22. C-DAC shall be under no obligation to accept the lowest or any tender and reserves the right of acceptance of the whole or any part of the tender. 

23. Any dispute arising out of this will be subject to the jurisdiction of the Court in Thiruvananthapuram.
24 The supplier shall take comprehensive insurance for all equipment supplied against any damages due to accidents, theft, sabotage or any other natural calamities like flood, lightning etc. The insurance coverage shall be valid till the delivery of the item at site. C-DAC shall not pay the supplier any additional cost in this regard. 

Section 2: Pre-Qualification Eligibility Criteria 
1. All firms participating in the bid must possess valid GST Registration Certificate. Bidder should be a company/firm/Proprietorship/Partnership registered in India. The documentary evidence for GST registration certificate / Income Tax Registration/ PAN number shall be provided to this effect. 

2. The bidder and OEM separately should submit an undertaking (In Original), clearly stating that they will facilitate on regular basis with technology / products updates & extend support during entire warranty period as mentioned in the tender document. 

3. The bidder should enclose General information of the bidder (Annexure - E) along with the bid. 

4. Bids should accompany the filled and signed Tender Document. 

5. Bid should accompany complete and signed copies of Annexures A, B, C, D, E, F, G & H. 

6. Bidder should submit tender specific Manufacturer’s Authorization Form (MAF) from OEM (Annexure- B) along with the bid. 

7. Bidder has to define a single point of contact for support and service related to all items covered in the tender. Contact details of the person to be submitted along with the bid.

8. The bidder should not have been barred or black-listed by any of the central/state govt departments/organizations/PSUs for any reason in the last three years. A self-declaration certificate from the authorized signatory should be submitted. 

9. Documentary proof for technical compliance should be submitted as per the technical specifications for all items given in this tender (Annexure -D). C-DAC reserves the right to verify, if it so desires, the correctness of documentary evidence furnished by the bidder. 

10. All the equipment supplied by the Bidder shall carry comprehensive on-site warranty for the entire contract period. The warranty will include all spares/accessories
11. If the Bidder fails to repair or replace the defective equipment/item, thenC-DAC will be free to get the same repaired/replaced from the market and its cost will be adjusted from the bidder’s performance security or recovered from the bidder.

12. Before submission of the bid, the bidders must verify the pre-qualification eligibility criteria and ensure fulfillment of all the terms and conditions. In the absence of documents / certificates under pre-qualification eligibility criteria above, the bid is liable to be rejected. 
13. The bidder should be an ARAI approved builder with a valid ARAI certificate. 

14. The body builder should be a legally valid registered entity located in Kerala for last 10 years.
15. The bidder should have built at least three mobile telemedicine units build on chassis of wheelbase more than 180 inch. Should enclose work orders/acceptance certificates of the three mobile medical units along with the technical bid.
16. The bidder should have Bus body design and approval of structure stability test according to the automotive Indian standard: AIS – 052
17. The bidder should have Bus body design and approval of the strength of Super structure test according to the Automotive Indian standard: AIS - 031

ANNEXURE A: TENDER ACCEPTANCE LETTER)

(To be given on Company Letter Head with sign and seal)
To: 







Date:

Section Head, Purchase

Centre for Development of Advanced Computing, 

P B No 6520, Vellayambalam, Thiruvananthapuram - 695033, Kerala 

Phone: +91 471 2723333 Ext 211; Mob: 7306701663
e-mail: purchase-cpp@cdac.in
Sub: Acceptance of Terms & Conditions of the Tender
Tender Reference No:…………………………………….
Name of Tender / Work: Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
Dear Sir,
1. I/We have downloaded  /  obtained  the  tender  document(s)  for  the  above mentioned `Tender/Work’  from  the web  site(s)  namely:  eprocure.gov.in/;  as given in the above mentioned website(s). 

2. I/We hereby certify  that  I  /  We  have  read  the  entire  terms  and  conditions  of  the tender documents  (including  all  documents  like  Annexure(s),  schedules(s), etc.), which form  part  of  the  contract agreement  and  I  /  We  shall  abide  hereby  by  the  terms  / conditions/ clauses contained therein. 

3. The corrigendum(s) issued from time to time by your department / organization should also be taken into consideration, while submitting this acceptance letter. 

4. I/We hereby unconditionally accept the  tender  conditions  of  above  mentioned  tender document(S) / corrigendum(s) in its totality / entirety. 

5. I/We do hereby declare that our Firm has not been blacklisted / debarred by any Govt. Department/Public sector undertaking 

 6.  I / We certify that all information  furnished by the our Firm is  true & correct and in  the event that   the   information   is   found   to    be   incorrect/untrue   or   found   violated,   then   your department/ organization shall without giving any notice or reason therefore or summarily  reject  the  bid  or terminate  the  contract, without  prejudice  to  any  other rights or remedy including  invocation of bid securing declaration.
Yours Faithfully, 
Authorized Signatory. 

(Signature of the Bidder, with Official Seal)

Annexure – B

MANUFACTURER AUTHORISATION FORMAT

(To be given on Manufacturer’s Letter Head with sign and seal)

To:










Date: 

Section Head, Purchase

Centre for Development of Advanced Computing,

P B No 6520, Vellayambalam, Thiruvananthapuram - 695033, Kerala

Phone: +91 471 2723333 Ext.211; Mob: 7306701663

e-mail: purchase-cpp@cdac.in
Tender Reference No:……………………

Subject:  Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
Dear Sir, 

We, M/s (Name of  the manufacturer)  having  registered  office  at  (address of  the manufacturer) hereby virtue of  being manufacturer  for  (Name of the product/s),  hereby  authorize M/s  (Name of the bidder) having their office at (Address of bidder) to submit quote, negotiate, supply,  install and  provide  after  sales  support  for  our  range  of products  quoted  by  them  to meet  the  above mentioned tender requirements at C-DAC, Thiruvananthapuram.

M/s (Name of the manufacturer) within the scope of requirement as per the tender mentioned above through    its   authorized   partner   M/s  (Name of  the  bidder)  shall  provide    support  &  product  warranty services for a minimum period of three  years from the date of acceptance of items.

The undersigned is authorized to issue such authorization on behalf of  M/s  (Name  of the manufacturer). 

For M/s (Name of the manufacturer) 

Signature & company seal 

Name

:

Designation
:

E-mail

:

Mobile No. 
:

Annexure - C

COMMERCIAL PRICE DECLARATION

(To be given on Company Letter Head with sign and seal)

Tender Reference No…………………………..

Bill of Quantities: 
	S. No.
	Description of Item 
	Qty.

	1
	Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
	2


Note: All the above items/system/modules including its Cables & Accessories need to  be supplied with 3 years on-site service & replaceable warranty for the smooth running of the respective system for the purpose for which it is been used/installed.
We……..………………………………………………………………………………………………………………………………… (Company Name) hereby certify that the total quoted price in the BOQ is “all-inclusive till destination”. The price quoted includes all other taxes, duties, packing& forwarding, freight, insurance, customs duty and allied clearance charges till destination/s as mentioned.    

Yours Faithfully, 

Authorized Signatory. 

(Signature of the Bidder, with Official Seal
Annexure -D
Detailed Technical Specification

1. Mobile Cancer Detection Units
Supply, Installation, and fabrication of 2 Nos. of Mobile Cancer Detection units for Medical College Goa and KGMU Lucknow with 3 year onsite warranty.
Specification of equipments and details of work
General

1. Fresh water tank (100 liters) and waste water tank  made in S.S (150 liters) below chassis

2. Side marker lamps on roof top – 4 nos.

3. Extra brake lights -4 nos.

4. Blinker lights – 4 nos

5. New decorative tail lights in the rear.

6. Horn 2 nos. 

7. Dickey – both sides.

8. Provision for fitting medical equipments with vibration mounts

9. Full painting with PU white paint and sticker work (CDAC will approve the sticker design)

10. 25 meters of power cable for drawing power from local supply.

11. All windows with sliding tinted glasses

12. Curtains for all windows.

13. 25KW air conditioner mounted on top of the vehicle.

14. AC ducted to driver cabin, surgery room, Laboratory.

15. Sliding ladder under door for patient entry.

16. Pneumatic power operated doors

17. Galvanized tubular structure with MIG welding 

Driver Cabin
1. New Modified front show with wind screen frame, wind screen glasses with rubber

2. New decorative headlights – 4 nos, heavy duty bumper

3. Halogen decorative lights below head lights

4. Fog lights -2nos, parking lights on front show grill

5. Driver, co-driver door 18/20 gauge super structure

6. Thermocole insulation for roof top, ceiling speakers

7. 18/20 gauge CRCA  MS Sheet for exterior upper portion , 20 gauge aluminum sheet for bottom portion and 3mm ACP panel for interior, with glossy ivory/white color

8. Fabrication of dashboard in colour coated sheet

9. Provision for fitment of dashboard meters

10. Fitting  Scania/Volvo type heavy duty wiper with water washer point

11. Vinyl sheet strip on the top and below the wind screen glass

12. Driver and co-driver doors window with 5mm clear glass with sliding arrangement- green tinted glass

13. Quarter glass for both sides for better view

14. Communication window on the partition behind driver

15. PVC vinyl sheet for flooring minimum 2mm thickness

16. Fitting of original driver seat. New reclining seat for co-driver, PVC handles 2 Nos

17. Fitting of original side mirrors , sun visors– 2 nos

18. Procurement and fitting of public address system+ amplifier

19. Procurement and fitting of LED TV Music system, wireless mic, Music players

20. Reverse camera unit

21. Fire extinguisher 1  

22. Ceiling speakers – 2 Nos.

23. 2 LAN port

24. Floor18mm Marine plywood
25. Height adjustable screen for separating driver seat and passenger seat

Cryosurgery room behind driver cabin
1. Procurement and fixing of Gynecology Surgery Table

2. Stool for doctor- revolving stool, movable 

3. Folding lamp on side of wall

4. 1 nos. chair and one folding table (refer diagram), one chair to rotate 180 degrees.

5. Overhead storage racks for storing the colposcope accessories and portable ultrasound machine.

6. Grilled bottom of the partition wall separating laboratory and driver cabin

7. 2 LAN port

Laboratory (2nd cabin from driver cabin)
1. Table for hematology  analyzer, sterilizer and biochemistry analyzer( refer diagram)

2. Fixing of refrigerator, UPS under table

3. One chair ( fixed) and one folding table for lap top

4. One moving chair

5. One wash basin- 304 grade stainless steel with 1mm thickness , quarter turn water tap and AC operated pressure pump

6. 3 Nos LAN ports

7. Granite table top
Mammography room / X-ray room (Right back end room)
1. 2 mm lead lined walls
2. Fixing of x-ray wall stand
3. Fixing of mammography unit
4. Fixing of CR unit
5. Corner curtain channel and curtain for dress change
6. Viewing window with lead glass.
7. Folding type bed with  PVC extruded foam top
8. 4 Nos LAN ports.
ELECTRICAL ITEMS (Total)

	Sl No
	Item
	Point
	Switch
	Power

	1. Driver Cum Passenger Cabin

	1
	LED 
	
	1
	Battery

	2
	LED
	
	1
	UPS

	3
	5/15 Plug
	2
	2
	UPS

	4
	Fan
	
	2
	UPS

	2. Cryosurgery Room

	5
	5/15 Plug for Laptop
	1
	1
	UPS

	6
	5/15 Plug for Laptop
	1
	1
	UPS

	7
	5/15 Plug for Colposcope unit
	1
	1
	UPS

	8
	5/15 Plug for Monitor
	1
	1
	UPS

	9
	5/15 Plug for AC
	1
	1
	UPS

	10
	5/15 Plug for ultrasound machine
	1
	1
	UPS

	11
	5/15 Plug Spare
	1
	1
	UPS

	12
	5/15 Plug Spare
	1
	1
	UPS

	13
	5/15 Plug Spare
	3
	3
	UPS

	14
	LED
	2
	2
	UPS

	15
	LED 
	1
	1
	Battery

	16
	Spot Light
	
	1
	UPS

	17
	Fan
	
	2
	UPS

	3. Laboratory

	18
	5/15 Plug for Microscope
	1
	1
	UPS

	19
	5/15 Plug for Biochemistry Analyzer
	1
	1
	UPS

	20
	5/15 Plug for Hematology Analyzer
	1
	1
	UPS

	21
	5/15 Plug for Refrigerator
	1
	1
	UPS

	22
	5/15 Plug for Sterilizer
	1
	1
	Mains

	23
	5/15 Plug for ECG
	2
	2
	UPS

	24
	5/15 Spare Plug
	1
	1
	Mains

	25
	LED
	2
	2
	UPS

	26
	LED 
	1
	1
	Battery

	27
	Spot Light
	
	1
	UPS

	29
	Fan
	
	2
	UPS

	30
	5/15 Plug for AC
	1
	1
	Mains

	4. Mammography Room

	31
	5/15 Plug For X-Ray
	1
	1
	Mains

	32
	5/15 Plug for Mammography unit
	1
	1
	Mains

	33
	5/15 Plug for CR unit
	1
	1
	UPS

	34
	5/15 Spare Plug
	1
	1
	UPS

	35
	5/15 Spare Plug
	2
	2
	UPS

	36
	5/15 Spare Plug
	1
	1
	Mains

	37
	Focusing Lamp
	1
	1
	UPS

	38
	5/15 Plug for AC
	1
	1
	Mains

	5. Others

	39
	MCB
	
	1
	Generator

	40
	MCB
	
	1
	Line /Gen

	41
	Changeover Switch
	
	1
	Line/Gen

	42
	25A,100mA ELCB for Plug Points / Cabin
	
	1
	UPS

	43
	25A,100mA ELCB for Lights
	
	1
	UPS

	44
	25A,100mA ELCB for Fans
	
	1
	UPS

	45
	25A,100mA ELCB for X-Ray
	
	1
	Mains

	46
	25A,100mA ELCB for AC and Sterilizer
	
	1
	Mains

	47
	25A,100mA ELCB for Mammography unit
	
	
	


1. Selector switch for choosing generator or Mains supply.

2. 6KVA UPS charging from petrol generator.

3. Batteries of UPS mounted on racks under chassis.

4. 25 meter cable to draw supply from local power supply with 16A male pin.

5. One ton split air conditioner in Surgery room, Laboratory and in X-ray room.

6. AC outdoor units mounted under chassis.

	#1
	Online UPS
	Quantity    2

	Sl. no.
	Item 
	Minimum Requirement 

	1
	Type
	Uninterruptible Power Supply (UPS)

	2
	Mode
	Online double conversion                                                        

	4
	Input voltage
	Input voltage range - 100 - 285V, Single phase

	5
	Output wave & Voltage
	sine wave  , 230V output, Single phase

	6
	Input Protection
	Circuit breaker

	7
	Efficiency at Full Load
	> 94%in double conversion mode, >98% in eco/Green mode

	8
	Output voltage capacity
	6 KVA

	9
	Battery
	External, 12V 42AH, SMF battery -16 Nos. make: Emerson/Quanta

	10
	Display
	LCD Display

	11
	Accessories
	Power cables ,battery rack, other accessories and interlinks

	12
	Dimensions
	Maximum 14.0cm (W) x 44.0cm (H) x 71.0cm (D)

	13
	Warranty
	3 year onsite warranty at Goa and Lucknow after installation


	#2
	Petrol Generator
	Quantity    2

	Sl. no.
	Item 
	Minimum Requirement 

	1
	Item
	Portable AC Generating Set Comprising Of Air Cooled 4 Stroke Single Cylinder Engine And Alternator

	2
	Starting and running
	Petrol start, Petrol run

	3
	Rated output
	5500 VA

	4
	Maximum Output
	7000 VA

	5
	Starting type 
	Push button Electric self start and Recoil

	7
	Fuel Tank capacity 
	19L

	8
	Power output 
	230 V AC

	9
	Dimension Of Generator In Mm LxWxH
	Maximum 1261x700x722

	10
	Maximum Weight (in kg)
	125

	11
	Frequency (Hz)
	50 

	12
	Warranty
	3 year onsite warranty at Goa and Lucknow after installation


	# 3
	Printer 
	Quantity    2

	Sl. No
	Item
	Description of Requirement

	1
	Print speed (A4)
	Upto 21ppm or higher

	2
	Print Resolution
	Upto 600x600 dpi

	3
	Print  Type
	Lasejet monochrome

	4
	Energy Star
	Supporting Energy star

	5
	Standard memory
	64 MB

	6
	Interface
	USB


	#4
	Automobile AC
	Quantity    2

	Sl. no.
	Item 
	Minimum Requirement 

	1
	Cooling capacity
	25KW

	2
	Compressor capacity
	300 or more

	3
	Refrigerant 
	R-134A

	4
	Supply voltage
	12/24 V

	5
	Current consumption
	<90A

	6
	Evaporator Type
	Inner grooved copper tubes & Hydrophilic Aluminium fins

	7
	Blower type
	Centrifugal type

	8
	Blower air flow
	4000 m3/h

	9
	No of blower
	4

	10
	Condenser type
	Inner grooved copper tubes & Aluminium fins

	11
	Fan type
	Axial type

	12
	Air flow
	6000 m3/h

	13
	No of fan
	3 or more

	14
	Warranty
	3 year onsite warranty at Goa and Lucknow after installation


	# 5
	AC -1 Ton
	Quantity    6

	Sl. no.
	Description / Technical specifications

	1
	Room Split Air Conditioner 1 Ton Inverter Technology, Consumption (Max) Watts: 1200. Min.  Copper condenser coil. BEEE star rating : 3star or above, Refrigerant – R 32

	2
	Automatic wall mountable stabilizer (voltage input range from 160V to 260V) suitable for 1 ton air conditioner. (ISO 9001 certified).

	5
	Extra interconnection copper pipe, electrical cable & suitable size drain pipe.


	# 6
	Extra items
	Quantity    

	1
	Folding Table 
	2

	2
	Stool
	6

	6
	16 Port Network Switch
	2


Annexure - E

General Information of the Bidder

(To be given on Company Letter Head with sign and seal)

	1.
	Name and address of the Supplier with 

Phone No. and E-Mail ID
	

	2.
	Registration Number and date of registration 
	

	3.
	Type of Organization 
	

	4.
	PAN Number (photocopy to be enclosed)
	

	5.
	GST Regn. No. 

(Number & photocopy of certificates to be given)
	

	6.
	Contact details of Single Point of Contact (SPOC) for support and service related to all items covered in the tender
	

	7.
	Additional information, if any 

(Attach separate sheet, if required)


	


Yours Faithfully, 

Authorized Signatory. 

(Signature of the Bidder, with Official Seal)

Annexure - F

Bid securing declaration

< In Bidders letter head >









Date:  [Insert: date of bid]

Tender No: …………………………..
From

(Registered name and address of the bidder) 

To:

Section Head, Purchase

Centre for Development of Advanced Computing,

P B No 6520, Vellayambalam, Thiruvananthapuram - 695033, Kerala

Phone: +91 471 2723333 Ext.211, +91-471-2723456

e-mail: purchase-cpp@cdac.in
Bid securing declaration

We, the undersigned on behalf of and under the authority of M/s ………………………… (herein after referred to as bidder) hereby undertakes to declare:

1. That we, the bidders understand that, bids can be supported with a Bid Securing Declaration, in lieu of submitting Earnest Money Deposit specified in the above referred tender and 

2. That we, the bidders, understand that we shall be automatically be suspended from being eligible for bidding in any contract with the Centre for Development of Advanced Computing(C-DAC) (herein after referred to as Purchaser) for a period of 3 years/or for a period as decided by the competent authority, commencing from the closing date of bid submission, on breach, by the bidder, of any of the following obligation(s) under the bid conditions:-

i. On withdrawal from the proposal or on enhancement of the quoted price subsequent to the bid opening and/or during the Bid validity period or of its extended period, if any.

ii. On failing to accept and/or execute the contract after being the successful bidder in accordance with the terms and conditions (including timelines for execution of the Agreement) of the said tender/Purchase Order issued thereof or on failure to furnish the performance security in accordance with the terms and conditions (including timelines for furnishing performance security) of the said tender/purchase order issued thereof.

iii. On indulging in any act that would jeopardize or unnecessarily delay the process of bid evaluation/finalization/execution of the proposed contract in accordance with timelines as specified by the purchaser. 

3. That we, the Bidders, understand that this declaration shall expire on our not being a successful Bidder and on notice of the award of the said contract to another Bidder or thirty days after the validity of the Bid; whichever matures earlier. 

(Signature)
Authorized Signatory 

Name

: __________________________________

Designation
: __________________________________

Office Seal
: __________________________________

Place              
: __________________________________

Date               
: __________________________________
Annexure - G

Certificate for Bidder Registration

(Ref: F.No.6/18/2019 – PPD dated 23rd July 2020)

< In Bidders letter head >

From









Date: ………. 

Tender No: ……………………….

(Registered name and address of the bidder) 

To:

Section Head, Purchase

Centre for Development of Advanced Computing,

P B No 6520, Vellayambalam, Thiruvananthapuram - 695033, Kerala

Phone: +91 471 2723333 Ext.211,Mob: 7306701663

e-mail: purchase-cpp@cdac.in
I have read the clause regarding restrictions on procurement from a bidder of a country which shares a land border with India; I certify that this bidder is not from such a country or, if from such a country, has been registered with the Competent Authority. I hereby certify that this bidder fulfills all requirements in this regard and is eligible to be considered. [Where applicable, evidence of valid registration by the Competent Authority shall be attached.]

(Signature) Authorized Signatory

Name
:




Designation: 

Office Seal: 

Place: 




Date:


Annexure – G
ITEMS SUPPLIED BY CDAC TO BODY BUILDER

	S. No.
	Description of Item 
	Qty.

	1
	Bus Chassis with Power Steering and front and rear Air Suspension
	2

	2
	Analog mammography machine with CR unit
	2

	3
	Portable Ultrasound system
	2

	4
	Digital X ray machine
	2

	5
	12 Lead Digital ECG Machine
	2

	6
	Hematology Analyser
	2

	7
	Digital Microscope
	2

	8
	HD Video Colposcope
	2

	9
	Cryo Surgery Unit+Nitrogen cylinders
	2

	10
	Table Top Sterilizer
	2

	11
	Laptop Computer
	2

	12
	Tool Kit
	2

	13
	Glucometer
	2

	14
	X Ray chest stand
	2

	
	
	

	15
	Weight & Height Measurement Instrument
	2

	16
	Pulse Oximeter
	2

	
	
	


Annexure – H

EQUIPMENTS TO BE PROCURE BY THE BODY BUILDER

	S. No.
	Description of Item 
	Qty.

	1
	Automobile AC
	2

	2
	50L Refrigerator
	2

	3
	7KVA Petrol Generator
	2

	4
	6KVA UPS with batteries
	2

	5
	One Ton inverter air conditioner
	6

	6
	Laserjet printer
	2

	7
	Stool 
	6

	8
	16 Port unmanaged Ethernet Switch
	2

	9
	Public address System with amplifier, microphone, DVD Player, 32” LED TV
	2

	10
	Table top autoclave
	2

	11
	Tool Kit 
	2

	12
	Fire Extinguisher
	2

	13
	First Aid Box
	2

	
	
	


